**LED Mini Magic Ball Light**

**USER’S MANUAL**

**Thanks for your choosing our product, please carefully read this manual and operate it obey the specification in order to make sure you can correct and safety installing, operating and maintaining it.**

**I. Technical Parameters**

Voltage: AC90-240V

Frequency: 50/60HZ

Power: 20W

Lamp: 6pcs LEDs

Controller Model: Auto, Sound Activate, DMX512 and Master-slave

Packing Size: 600 \*400 \*360mm(12pcs)

Net Weight: 0.6KG, Gross Weight: 0.8KG

**II. Menu Operation Instructions：**

Press **“Menu”** button to Set，to confirm by press **“ENTER”** button。correct by pressing **“UP&DOWN”** button.

|  |  |  |
| --- | --- | --- |
| **A001** | **001-512** | **Function Description** |
| A1-1 | A1-1～A1-9 | Red and Purple On Mode, Running Program speed from slow to fast |
| A2-1 | A2-1～A2-9 | Green and White On Mode, Running Program speed from slow to fast |
| A3-1 | A3-1～A3-9 | Blue and Yellow On Mode, Running Program speed from slow to fast |
| A4-1 | A4-1～A4-9 | Six color hopping mode, Running Program speed from slow to fast |
| A5-1 | A5-1～A5-9 | Gradient mode, Running Program speed from slow to fast |
| A6-1 | A6-1～A6-9 | Gradient mode, Running Program speed from slow to fast |
| A7-1 | A7-1～A7-9 | Strobe mode, Running Program speed from slow to fast |
| S1-1 | S1-1～S1-20 | Sound control strobe |
| S2-1 | S2-1～S1-20 | Sound control |

**III：DMX Channel Operations:**

|  |  |  |
| --- | --- | --- |
| **Channel** | **Channel values** | **Function Description** |
| CH1 | 0-255 | Dimming |
| CH2 | 0-255 | Red & purple LED dimming, brightness fade from dark |
| CH3 | 0-255 | Green& White LED dimming, brightness fade from dark |
| CH4 | 0-255 | Blue & Orange LED dimming, brightness fade from dark |
| CH5 | 0-255 | Strobe From fast to low |
| CH6 | 0-255 | Rotation |
| CH7 | 0-9 | No Function |
| 10-196 | Auto Program |
| 197-220 | Sound Control Strobe |
| 221-255 | Sound Control |